ADDENDUM TO 792

CHANGES IN SCOPE OF WORK:

Removal of dead branches and broken branches greater than 2” over the staked trail only.

* Invasive vines will be cut at the base of the tree.
* Stumps can be pushed into holes where possible and flush cut.